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1        National Geodetic Survey,   Retrieval Date = AUGUST  8, 2019
 BU1331 ***********************************************************************
 BU1331  DESIGNATION -  U 16
 BU1331  PID         -  BU1331
 BU1331  STATE/COUNTY-  AL/ESCAMBIA
 BU1331  COUNTRY     -  US
 BU1331  USGS QUAD   -  POLLARD (1986)
 BU1331
 BU1331                         *CURRENT SURVEY CONTROL
 BU1331  ______________________________________________________________________
 BU1331* NAD 83(1986) POSITION- 31 00 22.     (N) 087 14 25.     (W)   SCALED    
 BU1331* NAVD 88 ORTHO HEIGHT -    32.581 (meters)      106.89  (feet) ADJUSTED  
 BU1331  ______________________________________________________________________
 BU1331  GEOID HEIGHT    -        -27.828 (meters)                     GEOID12B
 BU1331  DYNAMIC HEIGHT  -         32.540 (meters)      106.76  (feet) COMP
 BU1331  MODELED GRAVITY -    979,383.7   (mgal)                       NAVD 88
 BU1331
 BU1331  VERT ORDER      -  FIRST     CLASS II
 BU1331
 BU1331.The horizontal coordinates were scaled from a topographic map and have
 BU1331.an estimated accuracy of +/- 6 seconds.
 BU1331.
 BU1331.The orthometric height was determined by differential leveling and
 BU1331.adjusted by the NATIONAL GEODETIC SURVEY
 BU1331.in June 1991.
 BU1331
 BU1331.Significant digits in the geoid height do not necessarily reflect accuracy.
 BU1331.GEOID12B height accuracy estimate available here.
 BU1331
 BU1331.The dynamic height is computed by dividing the NAVD 88
 BU1331.geopotential number by the normal gravity value computed on the
 BU1331.Geodetic Reference System of 1980 (GRS 80) ellipsoid at 45
 BU1331.degrees latitude (g = 980.6199 gals.).
 BU1331
 BU1331.The modeled gravity was interpolated from observed gravity values.
 BU1331
 BU1331;                    North         East    Units  Estimated Accuracy
 BU1331;SPC AL W     -   111,560.      624,800.      MT  (+/- 180 meters Scaled)
 BU1331
 BU1331_U.S. NATIONAL GRID SPATIAL ADDRESS: 16RDV770303(NAD 83)
 BU1331
 BU1331                          SUPERSEDED SURVEY CONTROL
 BU1331
 BU1331  NGVD 29 (??/??/92)   32.572  (m)          106.86   (f) ADJ UNCH    1 2
 BU1331
 BU1331.Superseded values are not recommended for survey control.
 BU1331
 BU1331.NGS no longer adjusts projects to the NAD 27 or NGVD 29 datums.
 BU1331.See file dsdata.pdf to determine how the superseded data were derived.
 BU1331
 BU1331_MARKER: DB = BENCH MARK DISK
 BU1331_SETTING: 7 = SET IN TOP OF CONCRETE MONUMENT
 BU1331_STAMPING: U 16 1934
 BU1331_STABILITY: C = MAY HOLD, BUT OF TYPE COMMONLY SUBJECT TO
 BU1331+STABILITY: SURFACE MOTION
 BU1331
 BU1331  HISTORY     - Date     Condition        Report By
 BU1331  HISTORY     - 1934     MONUMENTED       CGS
 BU1331  HISTORY     - 1955     GOOD             CGS
 BU1331
 BU1331                          STATION DESCRIPTION
 BU1331
 BU1331'DESCRIBED BY COAST AND GEODETIC SURVEY 1955
 BU1331'1.3 MI NE FROM FLOMATON.
 BU1331'1.3 MILES NORTHEAST ALONG THE LOUISVILLE AND NASHVILLE RAILROAD FROM
 BU1331'THE STATION AT FLOMATON, ABOUT 1.2 MILES SOUTH OF THE OVERPASS OF U.S.
 BU1331'HIGHWAY 31 OVER THE TRACKS, ABOUT 0.2 MILE NORTHEAST OF MILE POST 608,
 BU1331'AT AN EAST-WEST DIRT ROAD CROSSING, 40 FEET NORTHWEST OF NORTHWEST
 BU1331'RAIL, 74 FEET NORTH OF CENTER OF CROSSING, 57 FEET NORTH OF CENTER OF
 BU1331'A CATTLE GUARD ACROSS TRACK, 40 1/2 FEET WEST-SOUTHWEST OF TELEPHONE
 BU1331'POLE NO. 3209, 7 FEET SOUTHEAST OF A FENCE LINE, 21 FEET NORTHEAST OF
 BU1331'A FENCE CORNER, 51 FEET NORTH OF NORTHEAST END OF AN 18-INCH TILE PIPE
 BU1331'CULVERT UNDER ROAD, ABOUT 2 FEET ABOVE LEVEL OF TRACK AND SET IN THE
 BU1331'TOP OF A CONCRETE POST PROJECTING 1 INCH.







































1        National Geodetic Survey,   Retrieval Date = AUGUST  8, 2019
 BU1330 ***********************************************************************
 BU1330  DESIGNATION -  T 16
 BU1330  PID         -  BU1330
 BU1330  STATE/COUNTY-  AL/ESCAMBIA
 BU1330  COUNTRY     -  US
 BU1330  USGS QUAD   -  POLLARD (1986)
 BU1330
 BU1330                         *CURRENT SURVEY CONTROL
 BU1330  ______________________________________________________________________
 BU1330* NAD 83(1986) POSITION- 31 02 18.     (N) 087 13 44.     (W)   SCALED    
 BU1330* NAVD 88 ORTHO HEIGHT -    35.072 (meters)      115.07  (feet) ADJUSTED  
 BU1330  ______________________________________________________________________
 BU1330  GEOID HEIGHT    -        -27.826 (meters)                     GEOID12B
 BU1330  DYNAMIC HEIGHT  -         35.028 (meters)      114.92  (feet) COMP
 BU1330  MODELED GRAVITY -    979,381.0   (mgal)                       NAVD 88
 BU1330
 BU1330  VERT ORDER      -  SECOND    CLASS 0
 BU1330
 BU1330.The horizontal coordinates were scaled from a topographic map and have
 BU1330.an estimated accuracy of +/- 6 seconds.
 BU1330.
 BU1330.The orthometric height was determined by differential leveling and
 BU1330.adjusted by the NATIONAL GEODETIC SURVEY
 BU1330.in June 1991.
 BU1330
 BU1330.Significant digits in the geoid height do not necessarily reflect accuracy.
 BU1330.GEOID12B height accuracy estimate available here.
 BU1330
 BU1330.The dynamic height is computed by dividing the NAVD 88
 BU1330.geopotential number by the normal gravity value computed on the
 BU1330.Geodetic Reference System of 1980 (GRS 80) ellipsoid at 45
 BU1330.degrees latitude (g = 980.6199 gals.).
 BU1330
 BU1330.The modeled gravity was interpolated from observed gravity values.
 BU1330
 BU1330;                    North         East    Units  Estimated Accuracy
 BU1330;SPC AL W     -   115,140.      625,880.      MT  (+/- 180 meters Scaled)
 BU1330
 BU1330_U.S. NATIONAL GRID SPATIAL ADDRESS: 16RDV781338(NAD 83)
 BU1330
 BU1330                          SUPERSEDED SURVEY CONTROL
 BU1330
 BU1330  NGVD 29 (??/??/92)   35.073  (m)          115.07   (f) ADJ UNCH    2 0
 BU1330
 BU1330.Superseded values are not recommended for survey control.
 BU1330
 BU1330.NGS no longer adjusts projects to the NAD 27 or NGVD 29 datums.
 BU1330.See file dsdata.pdf to determine how the superseded data were derived.
 BU1330
 BU1330_MARKER: DB = BENCH MARK DISK
 BU1330_SETTING: 7 = SET IN TOP OF CONCRETE MONUMENT
 BU1330_STAMPING: T 16 1934
 BU1330_STABILITY: C = MAY HOLD, BUT OF TYPE COMMONLY SUBJECT TO
 BU1330+STABILITY: SURFACE MOTION
 BU1330
 BU1330  HISTORY     - Date     Condition        Report By
 BU1330  HISTORY     - 1934     MONUMENTED       CGS
 BU1330  HISTORY     - 1955     GOOD             CGS
 BU1330
 BU1330                          STATION DESCRIPTION
 BU1330
 BU1330'DESCRIBED BY COAST AND GEODETIC SURVEY 1955
 BU1330'3.8 MI N FROM FLOMATON.
 BU1330'3.8 MILES NORTHEAST AND NORTH ALONG THE LOUISVILLE AND NASHVILLE
 BU1330'RAILROAD FROM THE STATION AT FLOMATON, 20 TELEPHONE POLES SOUTH OF A
 BU1330'GRAVEL ROAD CROSSING, 54 1/2 RAILS SOUTH OF MILE POST 611, AT A DIM
 BU1330'PRIVATE ROAD CROSSING WHICH LEADS TO A HOUSE ON EAST SIDE OF TRACK, 44
 BU1330'FEET EAST OF EAST RAIL, 63 FEET NORTHEAST OF CENTER OF CROSSING, 99
 BU1330'FEET EAST-SOUTHEAST AND ACROSS TRACK FROM TELEPHONE POLE NO. 3130, 56
 BU1330'FEET NORTHEAST OF CENTER OF A CATTLE GUARD ACROSS RAILROAD, 4 FEET
 BU1330'NORTH OF A CORNER FENCE POST, 2 FEET WEST OF A FENCE LINE, ABOUT 1
 BU1330'FOOT ABOVE LEVEL OF TRACK AND SET IN THE TOP OF A CONCRETE POST
 BU1330'PROJECTING 6 INCHES.








































1        National Geodetic Survey,   Retrieval Date = AUGUST  8, 2019
 BU1328 ***********************************************************************
 BU1328  DESIGNATION -  R 16
 BU1328  PID         -  BU1328
 BU1328  STATE/COUNTY-  AL/ESCAMBIA
 BU1328  COUNTRY     -  US
 BU1328  USGS QUAD   -  POLLARD (1986)
 BU1328
 BU1328                         *CURRENT SURVEY CONTROL
 BU1328  ______________________________________________________________________
 BU1328* NAD 83(1986) POSITION- 31 06 54.     (N) 087 13 26.     (W)   SCALED    
 BU1328* NAVD 88 ORTHO HEIGHT -    32.899 (meters)      107.94  (feet) ADJUSTED  
 BU1328  ______________________________________________________________________
 BU1328  GEOID HEIGHT    -        -27.849 (meters)                     GEOID12B
 BU1328  DYNAMIC HEIGHT  -         32.858 (meters)      107.80  (feet) COMP
 BU1328  MODELED GRAVITY -    979,387.6   (mgal)                       NAVD 88
 BU1328
 BU1328  VERT ORDER      -  SECOND    CLASS 0
 BU1328
 BU1328.The horizontal coordinates were scaled from a topographic map and have
 BU1328.an estimated accuracy of +/- 6 seconds.
 BU1328.
 BU1328.The orthometric height was determined by differential leveling and
 BU1328.adjusted by the NATIONAL GEODETIC SURVEY
 BU1328.in June 1991.
 BU1328
 BU1328.Significant digits in the geoid height do not necessarily reflect accuracy.
 BU1328.GEOID12B height accuracy estimate available here.
 BU1328
 BU1328.The dynamic height is computed by dividing the NAVD 88
 BU1328.geopotential number by the normal gravity value computed on the
 BU1328.Geodetic Reference System of 1980 (GRS 80) ellipsoid at 45
 BU1328.degrees latitude (g = 980.6199 gals.).
 BU1328
 BU1328.The modeled gravity was interpolated from observed gravity values.
 BU1328
 BU1328;                    North         East    Units  Estimated Accuracy
 BU1328;SPC AL W     -   123,640.      626,340.      MT  (+/- 180 meters Scaled)
 BU1328
 BU1328_U.S. NATIONAL GRID SPATIAL ADDRESS: 16RDV786423(NAD 83)
 BU1328
 BU1328                          SUPERSEDED SURVEY CONTROL
 BU1328
 BU1328  NGVD 29 (??/??/92)   32.901  (m)          107.94   (f) ADJ UNCH    2 0
 BU1328
 BU1328.Superseded values are not recommended for survey control.
 BU1328
 BU1328.NGS no longer adjusts projects to the NAD 27 or NGVD 29 datums.
 BU1328.See file dsdata.pdf to determine how the superseded data were derived.
 BU1328
 BU1328_MARKER: DB = BENCH MARK DISK
 BU1328_SETTING: 7 = SET IN TOP OF CONCRETE MONUMENT
 BU1328_STAMPING: R 16 1934
 BU1328_STABILITY: C = MAY HOLD, BUT OF TYPE COMMONLY SUBJECT TO
 BU1328+STABILITY: SURFACE MOTION
 BU1328
 BU1328  HISTORY     - Date     Condition        Report By
 BU1328  HISTORY     - 1934     MONUMENTED       CGS
 BU1328  HISTORY     - 1955     GOOD             CGS
 BU1328
 BU1328                          STATION DESCRIPTION
 BU1328
 BU1328'DESCRIBED BY COAST AND GEODETIC SURVEY 1955
 BU1328'6.6 MI S FROM WALLACE.
 BU1328'6.6 MILES SOUTH ALONG THE LOUISVILLE AND NASHVILLE RAILROAD FROM THE
 BU1328'STATION AT WALLACE, ABOUT 9.1 MILES NORTH OF THE STATION AT FLOMATON,
 BU1328'556 FEET SOUTH OF CENTER OF CROSSING OF BLACK TOP ROAD AT FOSHEE, 42
 BU1328'1/2 FEET EAST OF EAST RAIL, 283 FEET NORTH-NORTHEAST OF NORTHEAST
 BU1328'CORNER OF TRESTLE NO. 10 OVER NARROW GAP CREEK, 42 FEET SOUTHEAST OF
 BU1328'MILE POST 616, 75 1/2 FEET EAST AND ACROSS TRACK FROM TELEPHONE POLE
 BU1328'NO. 2982, 3 1/2 FEET WEST OF A FENCE LINE, ABOUT 1 1/2 FEET ABOVE
 BU1328'LEVEL OF TRACK AND SET IN THE TOP OF A CONCRETE POST PROJECTING 3
 BU1328'INCHES.









































1        National Geodetic Survey,   Retrieval Date = AUGUST  8, 2019
 BU1325 ***********************************************************************
 BU1325  DESIGNATION -  N 16
 BU1325  PID         -  BU1325
 BU1325  STATE/COUNTY-  AL/ESCAMBIA
 BU1325  COUNTRY     -  US
 BU1325  USGS QUAD   -  WALLACE (1986)
 BU1325
 BU1325                         *CURRENT SURVEY CONTROL
 BU1325  ______________________________________________________________________
 BU1325* NAD 83(1986) POSITION- 31 12 32.     (N) 087 13 07.     (W)   SCALED    
 BU1325* NAVD 88 ORTHO HEIGHT -    50.869 (meters)      166.89  (feet) ADJUSTED  
 BU1325  ______________________________________________________________________
 BU1325  GEOID HEIGHT    -        -27.879 (meters)                     GEOID12B
 BU1325  DYNAMIC HEIGHT  -         50.805 (meters)      166.68  (feet) COMP
 BU1325  MODELED GRAVITY -    979,386.0   (mgal)                       NAVD 88
 BU1325
 BU1325  VERT ORDER      -  SECOND    CLASS 0
 BU1325
 BU1325.The horizontal coordinates were scaled from a topographic map and have
 BU1325.an estimated accuracy of +/- 6 seconds.
 BU1325.
 BU1325.The orthometric height was determined by differential leveling and
 BU1325.adjusted by the NATIONAL GEODETIC SURVEY
 BU1325.in June 1991.
 BU1325
 BU1325.Significant digits in the geoid height do not necessarily reflect accuracy.
 BU1325.GEOID12B height accuracy estimate available here.
 BU1325
 BU1325.The dynamic height is computed by dividing the NAVD 88
 BU1325.geopotential number by the normal gravity value computed on the
 BU1325.Geodetic Reference System of 1980 (GRS 80) ellipsoid at 45
 BU1325.degrees latitude (g = 980.6199 gals.).
 BU1325
 BU1325.The modeled gravity was interpolated from observed gravity values.
 BU1325
 BU1325;                    North         East    Units  Estimated Accuracy
 BU1325;SPC AL W     -   134,050.      626,810.      MT  (+/- 180 meters Scaled)
 BU1325
 BU1325_U.S. NATIONAL GRID SPATIAL ADDRESS: 16RDV791527(NAD 83)
 BU1325
 BU1325                          SUPERSEDED SURVEY CONTROL
 BU1325
 BU1325  NGVD 29 (??/??/92)   50.862  (m)          166.87   (f) ADJ UNCH    2 0
 BU1325
 BU1325.Superseded values are not recommended for survey control.
 BU1325
 BU1325.NGS no longer adjusts projects to the NAD 27 or NGVD 29 datums.
 BU1325.See file dsdata.pdf to determine how the superseded data were derived.
 BU1325
 BU1325_MARKER: DB = BENCH MARK DISK
 BU1325_SETTING: 7 = SET IN TOP OF CONCRETE MONUMENT
 BU1325_STAMPING: N 16 1934
 BU1325_STABILITY: C = MAY HOLD, BUT OF TYPE COMMONLY SUBJECT TO
 BU1325+STABILITY: SURFACE MOTION
 BU1325
 BU1325  HISTORY     - Date     Condition        Report By
 BU1325  HISTORY     - 1934     MONUMENTED       CGS
 BU1325  HISTORY     - 1955     GOOD             CGS
 BU1325
 BU1325                          STATION DESCRIPTION
 BU1325
 BU1325'DESCRIBED BY COAST AND GEODETIC SURVEY 1955
 BU1325'IN WALLACE.
 BU1325'AT WALLACE, ALONG THE LOUISVILLE AND NASHVILLE RAILROAD, 311 FEET
 BU1325'SOUTH OF CENTER OF CROSSING OF A BLACK TOP ROAD, 24 1/2 FEET EAST OF
 BU1325'EAST RAIL, 85 FEET NORTH OF NORTHEAST CORNER OF THE STATION, 34 FEET
 BU1325'WEST OF A 40-INCH OAK TREE, 112 FEET SOUTHEAST AND ACROSS TRACK FROM
 BU1325'TELEPHONE POLE NO. 2801, IN THE WEST EDGE OF A DRIVE LEADING TO THE
 BU1325'STATION AND ON PAST THE EAST SIDE OF STATION, ABOUT 1 FOOT ABOVE LEVEL
 BU1325'OF TRACK AND SET IN THE TOP OF A CONCRETE POST PROJECTING 4 INCHES
 BU1325'ABOVE A SMALL MOUND OF DIRT LEFT INTACT BY GRADING OF DRIVE.










































1        National Geodetic Survey,   Retrieval Date = AUGUST  8, 2019
 BU1324 ***********************************************************************
 BU1324  DESIGNATION -  M 16
 BU1324  PID         -  BU1324
 BU1324  STATE/COUNTY-  AL/ESCAMBIA
 BU1324  COUNTRY     -  US
 BU1324  USGS QUAD   -  WALLACE (1986)
 BU1324
 BU1324                         *CURRENT SURVEY CONTROL
 BU1324  ______________________________________________________________________
 BU1324* NAD 83(1986) POSITION- 31 14 31.     (N) 087 13 11.     (W)   SCALED    
 BU1324* NAVD 88 ORTHO HEIGHT -    50.256 (meters)      164.88  (feet) ADJUSTED  
 BU1324  ______________________________________________________________________
 BU1324  GEOID HEIGHT    -        -27.892 (meters)                     GEOID12B
 BU1324  DYNAMIC HEIGHT  -         50.192 (meters)      164.67  (feet) COMP
 BU1324  MODELED GRAVITY -    979,386.7   (mgal)                       NAVD 88
 BU1324
 BU1324  VERT ORDER      -  SECOND    CLASS 0
 BU1324
 BU1324.The horizontal coordinates were scaled from a topographic map and have
 BU1324.an estimated accuracy of +/- 6 seconds.
 BU1324.
 BU1324.The orthometric height was determined by differential leveling and
 BU1324.adjusted by the NATIONAL GEODETIC SURVEY
 BU1324.in June 1991.
 BU1324
 BU1324.Significant digits in the geoid height do not necessarily reflect accuracy.
 BU1324.GEOID12B height accuracy estimate available here.
 BU1324
 BU1324.The dynamic height is computed by dividing the NAVD 88
 BU1324.geopotential number by the normal gravity value computed on the
 BU1324.Geodetic Reference System of 1980 (GRS 80) ellipsoid at 45
 BU1324.degrees latitude (g = 980.6199 gals.).
 BU1324
 BU1324.The modeled gravity was interpolated from observed gravity values.
 BU1324
 BU1324;                    North         East    Units  Estimated Accuracy
 BU1324;SPC AL W     -   137,710.      626,700.      MT  (+/- 180 meters Scaled)
 BU1324
 BU1324_U.S. NATIONAL GRID SPATIAL ADDRESS: 16RDV790564(NAD 83)
 BU1324
 BU1324                          SUPERSEDED SURVEY CONTROL
 BU1324
 BU1324  NGVD 29 (??/??/92)   50.250  (m)          164.86   (f) ADJ UNCH    2 0
 BU1324
 BU1324.Superseded values are not recommended for survey control.
 BU1324
 BU1324.NGS no longer adjusts projects to the NAD 27 or NGVD 29 datums.
 BU1324.See file dsdata.pdf to determine how the superseded data were derived.
 BU1324
 BU1324_MARKER: DB = BENCH MARK DISK
 BU1324_SETTING: 7 = SET IN TOP OF CONCRETE MONUMENT
 BU1324_STAMPING: M 16 1934
 BU1324_STABILITY: C = MAY HOLD, BUT OF TYPE COMMONLY SUBJECT TO
 BU1324+STABILITY: SURFACE MOTION
 BU1324
 BU1324  HISTORY     - Date     Condition        Report By
 BU1324  HISTORY     - 1934     MONUMENTED       CGS
 BU1324  HISTORY     - 1955     GOOD             CGS
 BU1324
 BU1324                          STATION DESCRIPTION
 BU1324
 BU1324'DESCRIBED BY COAST AND GEODETIC SURVEY 1955
 BU1324'2.3 MI N FROM WALLACE.
 BU1324'2.3 MILES NORTH ALONG THE LOUISVILLE AND NASHVILLE RAILROAD FROM THE
 BU1324'STATION AT WALLACE, AT AN OLD ABANDONED ROAD CROSSING (VERY DIM), 43
 BU1324'FEET NORTHEAST OF NORTHEAST RAIL, ABOUT 100 FEET EAST OF CENTER OF OLD
 BU1324'CROSSING, 198 1/2 FEET SOUTHEAST OF MILE POST 625, 145 FEET SOUTHEAST
 BU1324'OF NORTHEAST END OF AN 18-INCH PIPE CULVERT UNDER TRACK, 74 FEET EAST
 BU1324'OF CENTER OF A CATTLE GUARD ACROSS TRACK, 87 1/2 FEET NORTH-NORTHEAST
 BU1324'AND ACROSS TRACK FROM TELEPHONE POLE NO. 2737, 35 FEET SOUTHEAST OF A
 BU1324'FENCE CORNER, 3 FEET SOUTHWEST OF A FENCE LINE, ABOUT 2 FEET BELOW
 BU1324'LEVEL OF TRACK AND SET IN THE TOP OF A CONCRETE POST PROJECTING 2
 BU1324'INCHES.








































1        National Geodetic Survey,   Retrieval Date = AUGUST  8, 2019
 BU1323 ***********************************************************************
 BU1323  DESIGNATION -  L 16
 BU1323  PID         -  BU1323
 BU1323  STATE/COUNTY-  AL/CONECUH
 BU1323  COUNTRY     -  US
 BU1323  USGS QUAD   -  RANGE (1971)
 BU1323
 BU1323                         *CURRENT SURVEY CONTROL
 BU1323  ______________________________________________________________________
 BU1323* NAD 83(1986) POSITION- 31 16 32.     (N) 087 14 07.     (W)   SCALED    
 BU1323* NAVD 88 ORTHO HEIGHT -    56.708 (meters)      186.05  (feet) ADJUSTED  
 BU1323  ______________________________________________________________________
 BU1323  GEOID HEIGHT    -        -27.915 (meters)                     GEOID12B
 BU1323  DYNAMIC HEIGHT  -         56.637 (meters)      185.82  (feet) COMP
 BU1323  MODELED GRAVITY -    979,386.7   (mgal)                       NAVD 88
 BU1323
 BU1323  VERT ORDER      -  SECOND    CLASS I
 BU1323
 BU1323.The horizontal coordinates were scaled from a topographic map and have
 BU1323.an estimated accuracy of +/- 6 seconds.
 BU1323.
 BU1323.The orthometric height was determined by differential leveling and
 BU1323.adjusted by the NATIONAL GEODETIC SURVEY
 BU1323.in June 1991.
 BU1323
 BU1323.Significant digits in the geoid height do not necessarily reflect accuracy.
 BU1323.GEOID12B height accuracy estimate available here.
 BU1323
 BU1323.The dynamic height is computed by dividing the NAVD 88
 BU1323.geopotential number by the normal gravity value computed on the
 BU1323.Geodetic Reference System of 1980 (GRS 80) ellipsoid at 45
 BU1323.degrees latitude (g = 980.6199 gals.).
 BU1323
 BU1323.The modeled gravity was interpolated from observed gravity values.
 BU1323
 BU1323;                    North         East    Units  Estimated Accuracy
 BU1323;SPC AL W     -   141,430.      625,210.      MT  (+/- 180 meters Scaled)
 BU1323
 BU1323_U.S. NATIONAL GRID SPATIAL ADDRESS: 16RDV776601(NAD 83)
 BU1323
 BU1323                          SUPERSEDED SURVEY CONTROL
 BU1323
 BU1323  NGVD 29 (??/??/92)   56.701  (m)          186.03   (f) ADJ UNCH    2 0
 BU1323
 BU1323.Superseded values are not recommended for survey control.
 BU1323
 BU1323.NGS no longer adjusts projects to the NAD 27 or NGVD 29 datums.
 BU1323.See file dsdata.pdf to determine how the superseded data were derived.
 BU1323
 BU1323_MARKER: DB = BENCH MARK DISK
 BU1323_SETTING: 7 = SET IN TOP OF CONCRETE MONUMENT
 BU1323_STAMPING: L 16 1934
 BU1323_MARK LOGO: CGS
 BU1323_MAGNETIC: O = OTHER; SEE DESCRIPTION
 BU1323_STABILITY: C = MAY HOLD, BUT OF TYPE COMMONLY SUBJECT TO
 BU1323+STABILITY: SURFACE MOTION
 BU1323_SATELLITE: THE SITE LOCATION WAS REPORTED AS NOT SUITABLE FOR
 BU1323+SATELLITE: SATELLITE OBSERVATIONS - December 15, 2005
 BU1323
 BU1323  HISTORY     - Date     Condition        Report By
 BU1323  HISTORY     - 1934     MONUMENTED       CGS
 BU1323  HISTORY     - 1955     GOOD             CGS
 BU1323  HISTORY     - 20040412 GOOD             ALHD
 BU1323  HISTORY     - 20051215 GOOD             WOOLPT
 BU1323
 BU1323                          STATION DESCRIPTION
 BU1323
 BU1323'DESCRIBED BY COAST AND GEODETIC SURVEY 1955
 BU1323'2.45 MI S FROM DEER RANGE.
 BU1323'2.45 MILES SOUTH ALONG THE LOUISVILLE AND NASHVILLE RAILROAD FROM THE
 BU1323'ROAD CROSSING AT DEER RANGE, ABOUT 4.85 MILES NORTH OF THE STATION AT
 BU1323'WALLACE, ESCAMBIA COUNTY, AT A DIRT ROAD CROSSING, 41.6 FEET EAST OF
 BU1323'EAST RAIL, 118 FEET SOUTHEAST OF CENTER OF CROSSING, 5 FEET WEST OF A
 BU1323'FENCE LINE, 83 FEET EAST-NORTHEAST AND ACROSS TRACK FROM TELEPHONE
 BU1323'POLE NO. 2669, 10 FEET SOUTHWEST OF A 10-INCH OAK TREE, 8 FEET
 BU1323'NORTHWEST OF A 12-INCH PINE TREE, ABOUT 1 FOOT ABOVE LEVEL OF TRACK
 BU1323'AND SET IN THE TOP OF A CONCRETE POST ABOUT FLUSH WITH GROUND.
 BU1323
 BU1323                          STATION RECOVERY (2004)
 BU1323
 BU1323'RECOVERY NOTE BY ALABAMA HIGHWAY DEPARTMENT 2004 (RBC)
 BU1323'RECOVERED IN GOOD CONDITION.
 BU1323
 BU1323                          STATION RECOVERY (2005)
 BU1323
 BU1323'RECOVERY NOTE BY WOOLPERT CONSULTANTS 2005 (ARL)
 BU1323'RECOVERED AS DESCRIBED.


























1        National Geodetic Survey,   Retrieval Date = AUGUST  8, 2019
 BU1321 ***********************************************************************
 BU1321  DESIGNATION -  J 16
 BU1321  PID         -  BU1321
 BU1321  STATE/COUNTY-  AL/CONECUH
 BU1321  COUNTRY     -  US
 BU1321  USGS QUAD   -  RANGE (1971)
 BU1321
 BU1321                         *CURRENT SURVEY CONTROL
 BU1321  ______________________________________________________________________
 BU1321* NAD 83(1986) POSITION- 31 20 29.     (N) 087 14 10.     (W)   SCALED    
 BU1321* NAVD 88 ORTHO HEIGHT -    97.796 (meters)      320.85  (feet) ADJUSTED  
 BU1321  ______________________________________________________________________
 BU1321  GEOID HEIGHT    -        -27.915 (meters)                     GEOID12B
 BU1321  DYNAMIC HEIGHT  -         97.673 (meters)      320.45  (feet) COMP
 BU1321  MODELED GRAVITY -    979,387.4   (mgal)                       NAVD 88
 BU1321
 BU1321  VERT ORDER      -  SECOND    CLASS I
 BU1321
 BU1321.The horizontal coordinates were scaled from a topographic map and have
 BU1321.an estimated accuracy of +/- 6 seconds.
 BU1321.
 BU1321.The orthometric height was determined by differential leveling and
 BU1321.adjusted by the NATIONAL GEODETIC SURVEY
 BU1321.in June 1991.
 BU1321
 BU1321.Significant digits in the geoid height do not necessarily reflect accuracy.
 BU1321.GEOID12B height accuracy estimate available here.
 BU1321
 BU1321.The dynamic height is computed by dividing the NAVD 88
 BU1321.geopotential number by the normal gravity value computed on the
 BU1321.Geodetic Reference System of 1980 (GRS 80) ellipsoid at 45
 BU1321.degrees latitude (g = 980.6199 gals.).
 BU1321
 BU1321.The modeled gravity was interpolated from observed gravity values.
 BU1321
 BU1321;                    North         East    Units  Estimated Accuracy
 BU1321;SPC AL W     -   148,730.      625,110.      MT  (+/- 180 meters Scaled)
 BU1321
 BU1321_U.S. NATIONAL GRID SPATIAL ADDRESS: 16RDV775674(NAD 83)
 BU1321
 BU1321                          SUPERSEDED SURVEY CONTROL
 BU1321
 BU1321  NGVD 29 (??/??/92)   97.779  (m)          320.80   (f) ADJ UNCH    2 0
 BU1321
 BU1321.Superseded values are not recommended for survey control.
 BU1321
 BU1321.NGS no longer adjusts projects to the NAD 27 or NGVD 29 datums.
 BU1321.See file dsdata.pdf to determine how the superseded data were derived.
 BU1321
 BU1321_MARKER: DB = BENCH MARK DISK
 BU1321_SETTING: 7 = SET IN TOP OF CONCRETE MONUMENT
 BU1321_STAMPING: J 16 1934
 BU1321_MARK LOGO: CGS
 BU1321_MAGNETIC: O = OTHER; SEE DESCRIPTION
 BU1321_STABILITY: C = MAY HOLD, BUT OF TYPE COMMONLY SUBJECT TO
 BU1321+STABILITY: SURFACE MOTION
 BU1321_SATELLITE: THE SITE LOCATION WAS REPORTED AS NOT SUITABLE FOR
 BU1321+SATELLITE: SATELLITE OBSERVATIONS - December 15, 2005
 BU1321
 BU1321  HISTORY     - Date     Condition        Report By
 BU1321  HISTORY     - 1934     MONUMENTED       CGS
 BU1321  HISTORY     - 1955     GOOD             CGS
 BU1321  HISTORY     - 20040412 GOOD             ALHD
 BU1321  HISTORY     - 20051215 GOOD             WOOLPT
 BU1321
 BU1321                          STATION DESCRIPTION
 BU1321
 BU1321'DESCRIBED BY COAST AND GEODETIC SURVEY 1955
 BU1321'4.75 MI S FROM REPTON.
 BU1321'4.75 MILES SOUTH ALONG THE LOUISVILLE AND NASHVILLE RAILROAD FROM THE
 BU1321'STATION AT REPTON, ABOUT 2.05 MILES NORTH OF THE ROAD CROSSING AT DEER
 BU1321'RANGE, ABOUT 0.15 MILE NORTH OF MILE POST 632, AT A SAND ROAD
 BU1321'CROSSING, 27 FEET WEST-SOUTHWEST OF NEAR RAIL, 64 FEET NORTHWEST OF
 BU1321'CENTER OF CROSSING, 18 FEET EAST-NORTHEAST OF CENTER LINE OF A SAND
 BU1321'ROAD PARALLEL TO TRACK, 75 FEET NORTH-NORTHEAST AND ACROSS ROAD FROM A
 BU1321'POWER POLE WHICH IS ON A BRANCH LINE, 9 1/2 FEET SOUTH-SOUTHEAST OF
 BU1321'TELEPHONE POLE NO. 2533, ABOUT 1/2 FOOT BELOW LEVEL OF TRACK AND SET
 BU1321'IN THE TOP OF A CONCRETE POST PROJECTING 2 INCHES.
 BU1321
 BU1321                          STATION RECOVERY (2004)
 BU1321
 BU1321'RECOVERY NOTE BY ALABAMA HIGHWAY DEPARTMENT 2004 (RBC)
 BU1321'RECOVERED IN GOOD CONDITION.
 BU1321
 BU1321                          STATION RECOVERY (2005)
 BU1321
 BU1321'RECOVERY NOTE BY WOOLPERT CONSULTANTS 2005 (ARL)
 BU1321'RECOVERED AS DESCRIBED.
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 BU1312 ***********************************************************************
 BU1312  DESIGNATION -  K 362
 BU1312  PID         -  BU1312
 BU1312  STATE/COUNTY-  AL/CONECUH
 BU1312  COUNTRY     -  US
 BU1312  USGS QUAD   -  REPTON (1986)
 BU1312
 BU1312                         *CURRENT SURVEY CONTROL
 BU1312  ______________________________________________________________________
 BU1312* NAD 83(1986) POSITION- 31 25 21.     (N) 087 14 22.     (W)   SCALED    
 BU1312* NAVD 88 ORTHO HEIGHT -   105.805 (meters)      347.13  (feet) ADJUSTED  
 BU1312  ______________________________________________________________________
 BU1312  GEOID HEIGHT    -        -27.878 (meters)                     GEOID12B
 BU1312  DYNAMIC HEIGHT  -        105.673 (meters)      346.70  (feet) COMP
 BU1312  MODELED GRAVITY -    979,393.7   (mgal)                       NAVD 88
 BU1312
 BU1312  VERT ORDER      -  SECOND    CLASS 0
 BU1312
 BU1312.The horizontal coordinates were scaled from a topographic map and have
 BU1312.an estimated accuracy of +/- 6 seconds.
 BU1312.
 BU1312.The orthometric height was determined by differential leveling and
 BU1312.adjusted by the NATIONAL GEODETIC SURVEY
 BU1312.in June 1991.
 BU1312
 BU1312.Significant digits in the geoid height do not necessarily reflect accuracy.
 BU1312.GEOID12B height accuracy estimate available here.
 BU1312
 BU1312.The dynamic height is computed by dividing the NAVD 88
 BU1312.geopotential number by the normal gravity value computed on the
 BU1312.Geodetic Reference System of 1980 (GRS 80) ellipsoid at 45
 BU1312.degrees latitude (g = 980.6199 gals.).
 BU1312
 BU1312.The modeled gravity was interpolated from observed gravity values.
 BU1312
 BU1312;                    North         East    Units  Estimated Accuracy
 BU1312;SPC AL W     -   157,720.      624,770.      MT  (+/- 180 meters Scaled)
 BU1312
 BU1312_U.S. NATIONAL GRID SPATIAL ADDRESS: 16RDV772764(NAD 83)
 BU1312
 BU1312                          SUPERSEDED SURVEY CONTROL
 BU1312
 BU1312  NGVD 29 (??/??/92)  105.790  (m)          347.08   (f) ADJ UNCH    2 0
 BU1312
 BU1312.Superseded values are not recommended for survey control.
 BU1312
 BU1312.NGS no longer adjusts projects to the NAD 27 or NGVD 29 datums.
 BU1312.See file dsdata.pdf to determine how the superseded data were derived.
 BU1312
 BU1312_MARKER: DB = BENCH MARK DISK
 BU1312_SETTING: 7 = SET IN TOP OF CONCRETE MONUMENT
 BU1312_STAMPING: K 362 1951
 BU1312_STABILITY: C = MAY HOLD, BUT OF TYPE COMMONLY SUBJECT TO
 BU1312+STABILITY: SURFACE MOTION
 BU1312
 BU1312  HISTORY     - Date     Condition        Report By
 BU1312  HISTORY     - 1951     MONUMENTED       CGS
 BU1312
 BU1312                          STATION DESCRIPTION
 BU1312
 BU1312'DESCRIBED BY COAST AND GEODETIC SURVEY 1951
 BU1312'1.0 MI N FROM REPTON.
 BU1312'1.0 MILE NORTH ALONG THE LOUISVILLE AND NASHVILLE RAILROAD FROM THE
 BU1312'STATION AT REPTON, 14 RAILS SOUTH OF MILE POST 638, AND SET AT THE
 BU1312'SOUTH END OF A SMALL DIRT CUT, 47 1/2 FEET EAST OF THE EAST RAIL, 1
 BU1312'FOOT EAST OF A FENCE LINE, 58 FEET WEST OF A 20-INCH HICKORY TREE WITH
 BU1312'FORKED TOP, ABOUT 2 FEET ABOVE THE TRACK AND SET IN THE TOP OF A
 BU1312'CONCRETE POST PROJECTING 4 INCHES.
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 BU1311 ***********************************************************************
 BU1311  DESIGNATION -  L 362
 BU1311  PID         -  BU1311
 BU1311  STATE/COUNTY-  AL/CONECUH
 BU1311  COUNTRY     -  US
 BU1311  USGS QUAD   -  REPTON (1986)
 BU1311
 BU1311                         *CURRENT SURVEY CONTROL
 BU1311  ______________________________________________________________________
 BU1311* NAD 83(1986) POSITION- 31 26 19.     (N) 087 14 28.     (W)   SCALED    
 BU1311* NAVD 88 ORTHO HEIGHT -   115.038 (meters)      377.42  (feet) ADJUSTED  
 BU1311  ______________________________________________________________________
 BU1311  GEOID HEIGHT    -        -27.867 (meters)                     GEOID12B
 BU1311  DYNAMIC HEIGHT  -        114.895 (meters)      376.95  (feet) COMP
 BU1311  MODELED GRAVITY -    979,397.2   (mgal)                       NAVD 88
 BU1311
 BU1311  VERT ORDER      -  SECOND    CLASS 0
 BU1311
 BU1311.The horizontal coordinates were scaled from a topographic map and have
 BU1311.an estimated accuracy of +/- 6 seconds.
 BU1311.
 BU1311.The orthometric height was determined by differential leveling and
 BU1311.adjusted by the NATIONAL GEODETIC SURVEY
 BU1311.in June 1991.
 BU1311
 BU1311.Significant digits in the geoid height do not necessarily reflect accuracy.
 BU1311.GEOID12B height accuracy estimate available here.
 BU1311
 BU1311.The dynamic height is computed by dividing the NAVD 88
 BU1311.geopotential number by the normal gravity value computed on the
 BU1311.Geodetic Reference System of 1980 (GRS 80) ellipsoid at 45
 BU1311.degrees latitude (g = 980.6199 gals.).
 BU1311
 BU1311.The modeled gravity was interpolated from observed gravity values.
 BU1311
 BU1311;                    North         East    Units  Estimated Accuracy
 BU1311;SPC AL W     -   159,510.      624,610.      MT  (+/- 180 meters Scaled)
 BU1311
 BU1311_U.S. NATIONAL GRID SPATIAL ADDRESS: 16RDV770782(NAD 83)
 BU1311
 BU1311                          SUPERSEDED SURVEY CONTROL
 BU1311
 BU1311  NGVD 29 (??/??/92)  115.021  (m)          377.36   (f) ADJ UNCH    2 0
 BU1311
 BU1311.Superseded values are not recommended for survey control.
 BU1311
 BU1311.NGS no longer adjusts projects to the NAD 27 or NGVD 29 datums.
 BU1311.See file dsdata.pdf to determine how the superseded data were derived.
 BU1311
 BU1311_MARKER: DB = BENCH MARK DISK
 BU1311_SETTING: 7 = SET IN TOP OF CONCRETE MONUMENT
 BU1311_STAMPING: L 362 1951
 BU1311_STABILITY: C = MAY HOLD, BUT OF TYPE COMMONLY SUBJECT TO
 BU1311+STABILITY: SURFACE MOTION
 BU1311
 BU1311  HISTORY     - Date     Condition        Report By
 BU1311  HISTORY     - 1951     MONUMENTED       CGS
 BU1311
 BU1311                          STATION DESCRIPTION
 BU1311
 BU1311'DESCRIBED BY COAST AND GEODETIC SURVEY 1951
 BU1311'2.1 MI N FROM REPTON.
 BU1311'2.1 MILES NORTH ALONG THE LOUISVILLE AND NASHVILLE RAILROAD FROM THE
 BU1311'STATION AT REPTON, IN THE SOUTHWEST QUARTER OF A DIRT ROAD CROSSING,
 BU1311'111 FEET NORTHWEST AND ACROSS TRACK FROM MILE POST 639, 26 FEET WEST
 BU1311'OF THE WEST RAIL, 30 FEET SOUTH OF THE CENTER LINE OF DIRT ROAD, 2 1/2
 BU1311'FEET SOUTH OF FIRST TELEPHONE POLE SOUTH OF ROAD CROSSING, 27 FEET
 BU1311'NORTHEAST OF A FENCE CORNER, ABOUT LEVEL WITH THE TRACK AND SET IN THE
 BU1311'TOP OF A CONCRETE POST PROJECTING 1 INCH.
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 BU1310 ***********************************************************************
 BU1310  DESIGNATION -  M 362
 BU1310  PID         -  BU1310
 BU1310  STATE/COUNTY-  AL/MONROE
 BU1310  COUNTRY     -  US
 BU1310  USGS QUAD   -  REPTON (1986)
 BU1310
 BU1310                         *CURRENT SURVEY CONTROL
 BU1310  ______________________________________________________________________
 BU1310* NAD 83(1986) POSITION- 31 27 09.     (N) 087 14 34.     (W)   SCALED    
 BU1310* NAVD 88 ORTHO HEIGHT -   112.516 (meters)      369.15  (feet) ADJUSTED  
 BU1310  ______________________________________________________________________
 BU1310  GEOID HEIGHT    -        -27.858 (meters)                     GEOID12B
 BU1310  DYNAMIC HEIGHT  -        112.376 (meters)      368.69  (feet) COMP
 BU1310  MODELED GRAVITY -    979,400.2   (mgal)                       NAVD 88
 BU1310
 BU1310  VERT ORDER      -  SECOND    CLASS 0
 BU1310
 BU1310.The horizontal coordinates were scaled from a topographic map and have
 BU1310.an estimated accuracy of +/- 6 seconds.
 BU1310.
 BU1310.The orthometric height was determined by differential leveling and
 BU1310.adjusted by the NATIONAL GEODETIC SURVEY
 BU1310.in June 1991.
 BU1310
 BU1310.Significant digits in the geoid height do not necessarily reflect accuracy.
 BU1310.GEOID12B height accuracy estimate available here.
 BU1310
 BU1310.The dynamic height is computed by dividing the NAVD 88
 BU1310.geopotential number by the normal gravity value computed on the
 BU1310.Geodetic Reference System of 1980 (GRS 80) ellipsoid at 45
 BU1310.degrees latitude (g = 980.6199 gals.).
 BU1310
 BU1310.The modeled gravity was interpolated from observed gravity values.
 BU1310
 BU1310;                    North         East    Units  Estimated Accuracy
 BU1310;SPC AL W     -   161,050.      624,450.      MT  (+/- 180 meters Scaled)
 BU1310
 BU1310_U.S. NATIONAL GRID SPATIAL ADDRESS: 16RDV769797(NAD 83)
 BU1310
 BU1310                          SUPERSEDED SURVEY CONTROL
 BU1310
 BU1310  NGVD 29 (??/??/92)  112.499  (m)          369.09   (f) ADJ UNCH    2 0
 BU1310
 BU1310.Superseded values are not recommended for survey control.
 BU1310
 BU1310.NGS no longer adjusts projects to the NAD 27 or NGVD 29 datums.
 BU1310.See file dsdata.pdf to determine how the superseded data were derived.
 BU1310
 BU1310_MARKER: DB = BENCH MARK DISK
 BU1310_SETTING: 7 = SET IN TOP OF CONCRETE MONUMENT
 BU1310_STAMPING: M 362 1951
 BU1310_STABILITY: C = MAY HOLD, BUT OF TYPE COMMONLY SUBJECT TO
 BU1310+STABILITY: SURFACE MOTION
 BU1310
 BU1310  HISTORY     - Date     Condition        Report By
 BU1310  HISTORY     - 1951     MONUMENTED       CGS
 BU1310
 BU1310                          STATION DESCRIPTION
 BU1310
 BU1310'DESCRIBED BY COAST AND GEODETIC SURVEY 1951
 BU1310'3.05 MI N FROM REPTON.
 BU1310'3.05 MILES NORTH ALONG THE LOUISVILLE AND NASHVILLE RAILROAD FROM THE
 BU1310'STATION AT REPTON, ABOUT 0.2 MILE SOUTH OF A GRAVEL ROAD CROSSING, AT
 BU1310'THE NORTH END OF AN OLD RAILROAD SIDING, 175 FEET SOUTH-SOUTHEAST AND
 BU1310'ACROSS TRACK FROM MILE POST 640, 20 FEET EAST OF THE EAST RAIL, 1 FOOT
 BU1310'EAST OF A FENCE LINE, ABOUT LEVEL WITH THE TRACK AND SET IN THE TOP OF
 BU1310'A CONCRETE POST PROJECTING 6 INCHES.
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 BU1308 ***********************************************************************
 BU1308  DESIGNATION -  E 16
 BU1308  PID         -  BU1308
 BU1308  STATE/COUNTY-  AL/MONROE
 BU1308  COUNTRY     -  US
 BU1308  USGS QUAD   -  REPTON (1986)
 BU1308
 BU1308                         *CURRENT SURVEY CONTROL
 BU1308  ______________________________________________________________________
 BU1308* NAD 83(1986) POSITION- 31 27 42.     (N) 087 14 37.     (W)   SCALED    
 BU1308* NAVD 88 ORTHO HEIGHT -   107.999 (meters)      354.33  (feet) ADJUSTED  
 BU1308  ______________________________________________________________________
 BU1308  GEOID HEIGHT    -        -27.852 (meters)                     GEOID12B
 BU1308  DYNAMIC HEIGHT  -        107.865 (meters)      353.89  (feet) COMP
 BU1308  MODELED GRAVITY -    979,402.2   (mgal)                       NAVD 88
 BU1308
 BU1308  VERT ORDER      -  SECOND    CLASS 0
 BU1308
 BU1308.The horizontal coordinates were scaled from a topographic map and have
 BU1308.an estimated accuracy of +/- 6 seconds.
 BU1308.
 BU1308.The orthometric height was determined by differential leveling and
 BU1308.adjusted by the NATIONAL GEODETIC SURVEY
 BU1308.in June 1991.
 BU1308
 BU1308.Significant digits in the geoid height do not necessarily reflect accuracy.
 BU1308.GEOID12B height accuracy estimate available here.
 BU1308
 BU1308.The dynamic height is computed by dividing the NAVD 88
 BU1308.geopotential number by the normal gravity value computed on the
 BU1308.Geodetic Reference System of 1980 (GRS 80) ellipsoid at 45
 BU1308.degrees latitude (g = 980.6199 gals.).
 BU1308
 BU1308.The modeled gravity was interpolated from observed gravity values.
 BU1308
 BU1308;                    North         East    Units  Estimated Accuracy
 BU1308;SPC AL W     -   162,070.      624,370.      MT  (+/- 180 meters Scaled)
 BU1308
 BU1308_U.S. NATIONAL GRID SPATIAL ADDRESS: 16RDV768807(NAD 83)
 BU1308
 BU1308                          SUPERSEDED SURVEY CONTROL
 BU1308
 BU1308  NGVD 29 (??/??/92)  107.981  (m)          354.27   (f) ADJ UNCH    2 0
 BU1308
 BU1308.Superseded values are not recommended for survey control.
 BU1308
 BU1308.NGS no longer adjusts projects to the NAD 27 or NGVD 29 datums.
 BU1308.See file dsdata.pdf to determine how the superseded data were derived.
 BU1308
 BU1308_MARKER: DB = BENCH MARK DISK
 BU1308_SETTING: 7 = SET IN TOP OF CONCRETE MONUMENT
 BU1308_STAMPING: E 16 1934
 BU1308_STABILITY: C = MAY HOLD, BUT OF TYPE COMMONLY SUBJECT TO
 BU1308+STABILITY: SURFACE MOTION
 BU1308
 BU1308  HISTORY     - Date     Condition        Report By
 BU1308  HISTORY     - 1934     MONUMENTED       CGS
 BU1308  HISTORY     - 1951     GOOD             CGS
 BU1308
 BU1308                          STATION DESCRIPTION
 BU1308
 BU1308'DESCRIBED BY COAST AND GEODETIC SURVEY 1951
 BU1308'3.75 MI N FROM REPTON.
 BU1308'3.75 MILES NORTH ALONG THE LOUISVILLE AND NASHVILLE RAILROAD FROM THE
 BU1308'STATION AT REPTON, ABOUT 0.3 MILE SOUTHWEST OF MILE POST 641, AT A
 BU1308'GRAVEL ROAD CROSSING (GRAVEL ROAD CROSSES TRACK TO THE EAST AND
 BU1308'PARALLELS THE TRACK TO NORTH), 33 1/2 FEET WEST OF THE WEST RAIL, 37
 BU1308'FEET EAST OF THE CENTER LINE OF GRAVEL ROAD PARALLELING TRACK, 64 FEET
 BU1308'NORTH OF THE FIRST TELEPHONE POLE NORTH OF CROSSING, 126 FEET
 BU1308'NORTHWEST OF THE CENTER OF THE CROSSING, 18 FEET EAST OF A FENCE LINE,
 BU1308'1 FOOT ABOVE THE TRACK AND SET IN THE TOP OF A CONCRETE POST
 BU1308'PROJECTING 2 INCHES.
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 BU1307 ***********************************************************************
 BU1307  DESIGNATION -  D 16
 BU1307  PID         -  BU1307
 BU1307  STATE/COUNTY-  AL/MONROE
 BU1307  COUNTRY     -  US
 BU1307  USGS QUAD   -  REPTON (1986)
 BU1307
 BU1307                         *CURRENT SURVEY CONTROL
 BU1307  ______________________________________________________________________
 BU1307* NAD 83(1986) POSITION- 31 29 36.     (N) 087 14 56.     (W)   SCALED    
 BU1307* NAVD 88 ORTHO HEIGHT -    75.585 (meters)      247.98  (feet) ADJUSTED  
 BU1307  ______________________________________________________________________
 BU1307  GEOID HEIGHT    -        -27.837 (meters)                     GEOID12B
 BU1307  DYNAMIC HEIGHT  -         75.492 (meters)      247.68  (feet) COMP
 BU1307  MODELED GRAVITY -    979,408.7   (mgal)                       NAVD 88
 BU1307
 BU1307  VERT ORDER      -  SECOND    CLASS 0
 BU1307
 BU1307.The horizontal coordinates were scaled from a topographic map and have
 BU1307.an estimated accuracy of +/- 6 seconds.
 BU1307.
 BU1307.The orthometric height was determined by differential leveling and
 BU1307.adjusted by the NATIONAL GEODETIC SURVEY
 BU1307.in June 1991.
 BU1307
 BU1307.Significant digits in the geoid height do not necessarily reflect accuracy.
 BU1307.GEOID12B height accuracy estimate available here.
 BU1307
 BU1307.The dynamic height is computed by dividing the NAVD 88
 BU1307.geopotential number by the normal gravity value computed on the
 BU1307.Geodetic Reference System of 1980 (GRS 80) ellipsoid at 45
 BU1307.degrees latitude (g = 980.6199 gals.).
 BU1307
 BU1307.The modeled gravity was interpolated from observed gravity values.
 BU1307
 BU1307;                    North         East    Units  Estimated Accuracy
 BU1307;SPC AL W     -   165,580.      623,860.      MT  (+/- 180 meters Scaled)
 BU1307
 BU1307_U.S. NATIONAL GRID SPATIAL ADDRESS: 16RDV763843(NAD 83)
 BU1307
 BU1307                          SUPERSEDED SURVEY CONTROL
 BU1307
 BU1307  NGVD 29 (??/??/92)   75.569  (m)          247.93   (f) ADJ UNCH    2 0
 BU1307
 BU1307.Superseded values are not recommended for survey control.
 BU1307
 BU1307.NGS no longer adjusts projects to the NAD 27 or NGVD 29 datums.
 BU1307.See file dsdata.pdf to determine how the superseded data were derived.
 BU1307
 BU1307_MARKER: DB = BENCH MARK DISK
 BU1307_SETTING: 7 = SET IN TOP OF CONCRETE MONUMENT
 BU1307_STAMPING: D 16 1934
 BU1307_STABILITY: C = MAY HOLD, BUT OF TYPE COMMONLY SUBJECT TO
 BU1307+STABILITY: SURFACE MOTION
 BU1307
 BU1307  HISTORY     - Date     Condition        Report By
 BU1307  HISTORY     - 1934     MONUMENTED       CGS
 BU1307
 BU1307                          STATION DESCRIPTION
 BU1307
 BU1307'DESCRIBED BY COAST AND GEODETIC SURVEY 1934
 BU1307'6.2 MI N FROM REPTON.
 BU1307'IN MONROE COUNTY, 6.2 MILES NORTH ALONG THE LOUISVILLE AND NASHVILLE
 BU1307'RAILROAD FROM THE STATION AT REPTON, CONECUH COUNTY, 11 RAILS NORTH OF
 BU1307'A ROAD CROSSING, 77 YARDS NORTH OF MILEPOST 643, 47 FEET EAST OF THE
 BU1307'CENTER LINE OF THE TRACK, AND 1 FOOT WEST OF THE RIGHT-OF-WAY FENCE. A
 BU1307'STANDARD DISK, STAMPED D 16 1934 AND SET IN THE TOP OF A CONCRETE
 BU1307'POST.
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 BU0817 ***********************************************************************
 BU0817  DESIGNATION -  A 26
 BU0817  PID         -  BU0817
 BU0817  STATE/COUNTY-  AL/MONROE
 BU0817  COUNTRY     -  US
 BU0817  USGS QUAD   -  MONROEVILLE (1986)
 BU0817
 BU0817                         *CURRENT SURVEY CONTROL
 BU0817  ______________________________________________________________________
 BU0817* NAD 83(1986) POSITION- 31 33 55.     (N) 087 16 56.     (W)   SCALED    
 BU0817* NAVD 88 ORTHO HEIGHT -    45.422 (meters)      149.02  (feet) ADJUSTED  
 BU0817  ______________________________________________________________________
 BU0817  GEOID HEIGHT    -        -27.814 (meters)                     GEOID12B
 BU0817  DYNAMIC HEIGHT  -         45.367 (meters)      148.84  (feet) COMP
 BU0817  MODELED GRAVITY -    979,420.5   (mgal)                       NAVD 88
 BU0817
 BU0817  VERT ORDER      -  SECOND    CLASS 0
 BU0817
 BU0817.The horizontal coordinates were scaled from a topographic map and have
 BU0817.an estimated accuracy of +/- 6 seconds.
 BU0817.
 BU0817.The orthometric height was determined by differential leveling and
 BU0817.adjusted by the NATIONAL GEODETIC SURVEY
 BU0817.in June 1991.
 BU0817
 BU0817.Significant digits in the geoid height do not necessarily reflect accuracy.
 BU0817.GEOID12B height accuracy estimate available here.
 BU0817
 BU0817.The dynamic height is computed by dividing the NAVD 88
 BU0817.geopotential number by the normal gravity value computed on the
 BU0817.Geodetic Reference System of 1980 (GRS 80) ellipsoid at 45
 BU0817.degrees latitude (g = 980.6199 gals.).
 BU0817
 BU0817.The modeled gravity was interpolated from observed gravity values.
 BU0817
 BU0817;                    North         East    Units  Estimated Accuracy
 BU0817;SPC AL W     -   173,550.      620,670.      MT  (+/- 180 meters Scaled)
 BU0817
 BU0817_U.S. NATIONAL GRID SPATIAL ADDRESS: 16RDV732922(NAD 83)
 BU0817
 BU0817                          SUPERSEDED SURVEY CONTROL
 BU0817
 BU0817  NGVD 29 (??/??/92)   45.406  (m)          148.97   (f) ADJ UNCH    2 0
 BU0817
 BU0817.Superseded values are not recommended for survey control.
 BU0817
 BU0817.NGS no longer adjusts projects to the NAD 27 or NGVD 29 datums.
 BU0817.See file dsdata.pdf to determine how the superseded data were derived.
 BU0817
 BU0817_MARKER: DB = BENCH MARK DISK
 BU0817_SETTING: 7 = SET IN TOP OF CONCRETE MONUMENT
 BU0817_STAMPING: A 26 1934
 BU0817_STABILITY: C = MAY HOLD, BUT OF TYPE COMMONLY SUBJECT TO
 BU0817+STABILITY: SURFACE MOTION
 BU0817
 BU0817  HISTORY     - Date     Condition        Report By
 BU0817  HISTORY     - 1934     MONUMENTED       CGS
 BU0817
 BU0817                          STATION DESCRIPTION
 BU0817
 BU0817'DESCRIBED BY COAST AND GEODETIC SURVEY 1934
 BU0817'2.3 MI NW FROM MONROETON STATION.
 BU0817'2.3 MILES NORTHWEST ALONG THE LOUISVILLE AND NASHVILLE RAILROAD FROM
 BU0817'THE STATION AT MONROETON, MONROE COUNTY, 4-2/3 RAILS SOUTH OF MILEPOST
 BU0817'649, AT A PRIVATED-ROAD CROSSING, 45.7 FEET WEST OF THE WEST RAIL, 19
 BU0817'FEET NORTH OF THE CENTER LINE OF THE PRIVATE FARM ROAD, 13.9 FEET
 BU0817'NORTH OF A RIGHT-OF-WAY FENCE CORNER, AND 2.5 FEET EAST OF THE
 BU0817'RIGHT-OF-WAY FENCE, AND SET IN THE TOP OF A CONCRETE POST PROJECTING 2
 BU0817'INCHES ABOVE GROUND.
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 BU0819 ***********************************************************************
 BU0819  DESIGNATION -  B 26
 BU0819  PID         -  BU0819
 BU0819  STATE/COUNTY-  AL/MONROE
 BU0819  COUNTRY     -  US
 BU0819  USGS QUAD   -  MONROEVILLE (1986)
 BU0819
 BU0819                         *CURRENT SURVEY CONTROL
 BU0819  ______________________________________________________________________
 BU0819* NAD 83(1986) POSITION- 31 35 13.     (N) 087 15 31.     (W)   SCALED    
 BU0819* NAVD 88 ORTHO HEIGHT -    54.394 (meters)      178.46  (feet) ADJUSTED  
 BU0819  ______________________________________________________________________
 BU0819  GEOID HEIGHT    -        -27.794 (meters)                     GEOID12B
 BU0819  DYNAMIC HEIGHT  -         54.327 (meters)      178.24  (feet) COMP
 BU0819  MODELED GRAVITY -    979,423.7   (mgal)                       NAVD 88
 BU0819
 BU0819  VERT ORDER      -  SECOND    CLASS 0
 BU0819
 BU0819.The horizontal coordinates were scaled from a topographic map and have
 BU0819.an estimated accuracy of +/- 6 seconds.
 BU0819.
 BU0819.The orthometric height was determined by differential leveling and
 BU0819.adjusted by the NATIONAL GEODETIC SURVEY
 BU0819.in June 1991.
 BU0819
 BU0819.Significant digits in the geoid height do not necessarily reflect accuracy.
 BU0819.GEOID12B height accuracy estimate available here.
 BU0819
 BU0819.The dynamic height is computed by dividing the NAVD 88
 BU0819.geopotential number by the normal gravity value computed on the
 BU0819.Geodetic Reference System of 1980 (GRS 80) ellipsoid at 45
 BU0819.degrees latitude (g = 980.6199 gals.).
 BU0819
 BU0819.The modeled gravity was interpolated from observed gravity values.
 BU0819
 BU0819;                    North         East    Units  Estimated Accuracy
 BU0819;SPC AL W     -   175,950.      622,910.      MT  (+/- 180 meters Scaled)
 BU0819
 BU0819_U.S. NATIONAL GRID SPATIAL ADDRESS: 16RDV754946(NAD 83)
 BU0819
 BU0819                          SUPERSEDED SURVEY CONTROL
 BU0819
 BU0819  NGVD 29 (??/??/92)   54.375  (m)          178.40   (f) ADJ UNCH    2 0
 BU0819
 BU0819.Superseded values are not recommended for survey control.
 BU0819
 BU0819.NGS no longer adjusts projects to the NAD 27 or NGVD 29 datums.
 BU0819.See file dsdata.pdf to determine how the superseded data were derived.
 BU0819
 BU0819_MARKER: DB = BENCH MARK DISK
 BU0819_SETTING: 7 = SET IN TOP OF CONCRETE MONUMENT
 BU0819_STAMPING: B 26 1934
 BU0819_STABILITY: C = MAY HOLD, BUT OF TYPE COMMONLY SUBJECT TO
 BU0819+STABILITY: SURFACE MOTION
 BU0819
 BU0819  HISTORY     - Date     Condition        Report By
 BU0819  HISTORY     - 1934     MONUMENTED       CGS
 BU0819  HISTORY     - 1951     GOOD             CGS
 BU0819
 BU0819                          STATION DESCRIPTION
 BU0819
 BU0819'DESCRIBED BY COAST AND GEODETIC SURVEY 1951
 BU0819'IN PETERMAN.
 BU0819'AT PETERMAN, ALONG THE LOUISVILLE AND NASHVILLE RAILROAD, 50 FEET
 BU0819'NORTH OF THE NORTHWEST CORNER OF STATION, 35 1/2 FEET WEST OF THE WEST
 BU0819'RAIL OF MAIN TRACK, 118 FEET SOUTHWEST OF THE SOUTHWEST CORNER OF
 BU0819'RAILROAD BRIDGE NO. 37C, ABOUT 2 FEET BELOW THE TRACK AND SET IN THE
 BU0819'TOP OF A CONCRETE POST PROJECTING 1 INCH.













































1        National Geodetic Survey,   Retrieval Date = AUGUST  8, 2019
 BU0821 ***********************************************************************
 BU0821  DESIGNATION -  C 26
 BU0821  PID         -  BU0821
 BU0821  STATE/COUNTY-  AL/MONROE
 BU0821  COUNTRY     -  US
 BU0821  USGS QUAD   -  BURNT CORN (1971)
 BU0821
 BU0821                         *CURRENT SURVEY CONTROL
 BU0821  ______________________________________________________________________
 BU0821* NAD 83(1986) POSITION- 31 36 38.     (N) 087 14 33.     (W)   SCALED    
 BU0821* NAVD 88 ORTHO HEIGHT -    69.768 (meters)      228.90  (feet) ADJUSTED  
 BU0821  ______________________________________________________________________
 BU0821  GEOID HEIGHT    -        -27.772 (meters)                     GEOID12B
 BU0821  DYNAMIC HEIGHT  -         69.684 (meters)      228.62  (feet) COMP
 BU0821  MODELED GRAVITY -    979,424.5   (mgal)                       NAVD 88
 BU0821
 BU0821  VERT ORDER      -  SECOND    CLASS 0
 BU0821
 BU0821.The horizontal coordinates were scaled from a topographic map and have
 BU0821.an estimated accuracy of +/- 6 seconds.
 BU0821.
 BU0821.The orthometric height was determined by differential leveling and
 BU0821.adjusted by the NATIONAL GEODETIC SURVEY
 BU0821.in June 1991.
 BU0821
 BU0821.Significant digits in the geoid height do not necessarily reflect accuracy.
 BU0821.GEOID12B height accuracy estimate available here.
 BU0821
 BU0821.The dynamic height is computed by dividing the NAVD 88
 BU0821.geopotential number by the normal gravity value computed on the
 BU0821.Geodetic Reference System of 1980 (GRS 80) ellipsoid at 45
 BU0821.degrees latitude (g = 980.6199 gals.).
 BU0821
 BU0821.The modeled gravity was interpolated from observed gravity values.
 BU0821
 BU0821;                    North         East    Units  Estimated Accuracy
 BU0821;SPC AL W     -   178,570.      624,430.      MT  (+/- 180 meters Scaled)
 BU0821
 BU0821_U.S. NATIONAL GRID SPATIAL ADDRESS: 16RDV769972(NAD 83)
 BU0821
 BU0821                          SUPERSEDED SURVEY CONTROL
 BU0821
 BU0821  NGVD 29 (??/??/92)   69.747  (m)          228.83   (f) ADJ UNCH    2 0
 BU0821
 BU0821.Superseded values are not recommended for survey control.
 BU0821
 BU0821.NGS no longer adjusts projects to the NAD 27 or NGVD 29 datums.
 BU0821.See file dsdata.pdf to determine how the superseded data were derived.
 BU0821
 BU0821_MARKER: DB = BENCH MARK DISK
 BU0821_SETTING: 7 = SET IN TOP OF CONCRETE MONUMENT
 BU0821_STAMPING: C 26 1934
 BU0821_STABILITY: C = MAY HOLD, BUT OF TYPE COMMONLY SUBJECT TO
 BU0821+STABILITY: SURFACE MOTION
 BU0821
 BU0821  HISTORY     - Date     Condition        Report By
 BU0821  HISTORY     - 1934     MONUMENTED       CGS
 BU0821  HISTORY     - 1951     GOOD             CGS
 BU0821
 BU0821                          STATION DESCRIPTION
 BU0821
 BU0821'DESCRIBED BY COAST AND GEODETIC SURVEY 1951
 BU0821'1.9 MI NE FROM PETERMAN.
 BU0821'ABOUT 1.9 MILES NORTHEAST ALONG THE LOUISVILLE AND NASHVILLE RAILROAD
 BU0821'FROM THE STATION AT PETERMAN, SET IN THE EAST QUARTER OF A PRIVATE
 BU0821'ROAD CROSSING, AT MILE POST 653, 28 FEET SOUTHEAST OF THE SOUTHEAST
 BU0821'RAIL, 24 FEET EAST OF THE MILE POST, 61 FEET NORTHEAST OF THE CENTER
 BU0821'LINE OF PRIVATE ROAD, 18 1/2 FEET NORTHWEST OF A FENCE LINE, ABOUT 2
 BU0821'FEET BELOW THE TRACK AND SET IN THE TOP OF A CONCRETE POST ABOUT 1
 BU0821'FOOT UNDER GROUND.
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 BU0823 ***********************************************************************
 BU0823  DESIGNATION -  H 355
 BU0823  PID         -  BU0823
 BU0823  STATE/COUNTY-  AL/MONROE
 BU0823  COUNTRY     -  US
 BU0823  USGS QUAD   -  BEATRICE (1981)
 BU0823
 BU0823                         *CURRENT SURVEY CONTROL
 BU0823  ______________________________________________________________________
 BU0823* NAD 83(1986) POSITION- 31 37 32.     (N) 087 14 32.     (W)   SCALED    
 BU0823* NAVD 88 ORTHO HEIGHT -    77.599 (meters)      254.59  (feet) ADJUSTED  
 BU0823  ______________________________________________________________________
 BU0823  GEOID HEIGHT    -        -27.764 (meters)                     GEOID12B
 BU0823  DYNAMIC HEIGHT  -         77.505 (meters)      254.28  (feet) COMP
 BU0823  MODELED GRAVITY -    979,425.9   (mgal)                       NAVD 88
 BU0823
 BU0823  VERT ORDER      -  SECOND    CLASS 0
 BU0823
 BU0823.The horizontal coordinates were scaled from a topographic map and have
 BU0823.an estimated accuracy of +/- 6 seconds.
 BU0823.
 BU0823.The orthometric height was determined by differential leveling and
 BU0823.adjusted by the NATIONAL GEODETIC SURVEY
 BU0823.in June 1991.
 BU0823
 BU0823.Significant digits in the geoid height do not necessarily reflect accuracy.
 BU0823.GEOID12B height accuracy estimate available here.
 BU0823
 BU0823.The dynamic height is computed by dividing the NAVD 88
 BU0823.geopotential number by the normal gravity value computed on the
 BU0823.Geodetic Reference System of 1980 (GRS 80) ellipsoid at 45
 BU0823.degrees latitude (g = 980.6199 gals.).
 BU0823
 BU0823.The modeled gravity was interpolated from observed gravity values.
 BU0823
 BU0823;                    North         East    Units  Estimated Accuracy
 BU0823;SPC AL W     -   180,240.      624,460.      MT  (+/- 180 meters Scaled)
 BU0823
 BU0823_U.S. NATIONAL GRID SPATIAL ADDRESS: 16RDV770989(NAD 83)
 BU0823
 BU0823                          SUPERSEDED SURVEY CONTROL
 BU0823
 BU0823  NGVD 29 (??/??/92)   77.581  (m)          254.53   (f) ADJ UNCH    2 0
 BU0823
 BU0823.Superseded values are not recommended for survey control.
 BU0823
 BU0823.NGS no longer adjusts projects to the NAD 27 or NGVD 29 datums.
 BU0823.See file dsdata.pdf to determine how the superseded data were derived.
 BU0823
 BU0823_MARKER: DB = BENCH MARK DISK
 BU0823_SETTING: 30 = SET IN A LIGHT STRUCTURE
 BU0823_SP_SET: CULVERT
 BU0823_STAMPING: H 355 1951
 BU0823_STABILITY: D = MARK OF QUESTIONABLE OR UNKNOWN STABILITY
 BU0823
 BU0823  HISTORY     - Date     Condition        Report By
 BU0823  HISTORY     - 1951     MONUMENTED       CGS
 BU0823
 BU0823                          STATION DESCRIPTION
 BU0823
 BU0823'DESCRIBED BY COAST AND GEODETIC SURVEY 1951
 BU0823'1.15 MI S FROM TUNNEL SPRINGS.
 BU0823'ABOUT 1.15 MILES SOUTH ALONG THE LOUISVILLE AND NASHVILLE RAILROAD
 BU0823'FROM THE STATION AT TUNNEL SPRINGS, 9 1/2 RAILS NORTH OF MILE POST
 BU0823'654, SET IN THE TOP AND DIRECTLY IN THE CENTER OF THE WEST END OF A
 BU0823'6-FOOT CONCRETE PIPE CULVERT (NO HEAD WALLS), 29 FEET WEST OF THE WEST
 BU0823'RAIL, 1 1/2 FEET EAST OF THE WEST END OF PIPE AND ABOUT 2 FEET BELOW
 BU0823'THE TRACK.
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